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Toughening modification of polylactic acid by long-chain hyperbranched polymers containing polycaprolactone end groups
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Fig. S1 Statistics of polylactic acid spherulite diameter.
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