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Effect of Acidic Media During the Hydrothermal Leaching of NiTi Alloy  
Highlights
· The hydrothermal leaching with HCl or H2SO4 acidic solutions are more efficient than those  with HNO3 or  H3PO4 acid solutions.

· Addition of hydrogen peroxide to HCl and H2SO4 acid solutions reduces the dissolution efficiency by increasing the oxide layer thickness at the alloy surface. 

· [bookmark: _GoBack]Nickel is more corroded than titanium within mineral acidic media.

