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	Parameter
	Pinion
	Crown

	
	Nominal diameter
	44 mm
	95 mm

	
	Teeth number
	44
	95

	
	Face width
	10 mm
	10 mm

	
	Superficial hardness
	230 HB
	230 HB

	
	Bending factor
	0.925
	1.0063

	
	Wear factor
	1.497
	2.2961


Source: Elaborated by the authors.
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