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Fig. S1 FTIR spectra of ss-CPCM3 before and after thermal cycling
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Fig. S2 FT-IR spectra of ss-CPCM3 and self-luminous ss-CPCM34
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