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Fig. S1 (a) The pristine CS-10 rubber grinding wheel and (b) CS-10 rubber grinding wheels exerting abrasion on WPU and its composite coatings.
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