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Abstract
[bookmark: _Hlk106013616]After delivering its sample capsule to Earth, the Hayabusa2 spacecraft started its extended mission to perform a flyby of asteroid 2001 CC21 in 2026 and rendezvous with asteroid 1998 KY26 in 2031. During the extended mission, the optical navigation camera (ONC) of Hayabusa2 will play an important role in navigation and science observations, but it has suffered from optical deterioration after the spacecraft’s surface contact with and sampling of asteroid Ryugu. Furthermore, the sensitivity of the telescopic camera (ONC-T) has continued to decrease for more than a year, posing a serious problem for the extended mission. These are problems that could potentially be encountered by other sample-return missions involving surface contact. In this study, we evaluated the long-term variation of ONC performance over the 6.5 years following the launch in 2014 to predict how it will perform during observations of the two target asteroids in its extended mission (6 and 11 years from the Earth return, respectively). Our results showed several important long-term trends in ONC performance, such as transmission, dark noise level, and hot pixels. During the long cruising period of the extended mission, we plan to observe both zodiacal light and exoplanet transits as additional science targets. The accuracy of these observations is sensitive to background noise level and stray-light contamination, so we conducted new test observations to search for the lowest stray light, which has been found to depend on spacecraft attitude. The results of these analyses and new test observations suggest that the Hayabusa2 ONC will be able to conduct cruising, flyby, and rendezvous observations of asteroids with sufficient accuracy.
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Introduction
After completing observations and sample collection of asteroid Ryugu from June 2018 to November 2019, Hayabusa2 successfully delivered Ryugu samples to Earth on December 6, 2020. Hayabusa2 then took off for another journey into deep space. JAXA is currently planning a flyby of the asteroid 2001 CC21 in July 2026 and a rendezvous with asteroid 1998 KY26 in July 2031 for the spacecraft’s extended mission (Hirabayashi et al., 2021; Mimasu et al., 2022).

The optical navigation camera (ONC) onboard Hayabusa2 is a two-dimensional charge-coupled device (CCD) camera system consisting of three camera heads: a telescopic camera with seven color filters (ONC-T), and two monochrome wide-angle cameras (ONC-W1, W2) (Kameda et al., 2015; Kameda et al., 2017; Suzuki et al., 2018; Tatsumi et al., 2019). These cameras have so far observed spectroscopic and morphologic properties of asteroid Ryugu (e.g., Sugita et al., 2019; Watanabe et al., 2019; Tatsumi et al., 2020; Yokota et al., 2021), dynamic processes during the touchdown (TD) sequences (Morota et al., 2020; Tachibana et al., 2022), and the artificially generated crater on Ryugu (e.g., Arakawa et al., 2020; Honda et al., 2021). The ONC will also be used to observe the shape, morphology, and spectra of the target asteroids during the extended mission. However, post-TD health-check observations have shown that the optical performance of the ONC has degraded, most likely because of the adhesion of surface materials kicked up during the two TDs on Ryugu’s surface (Figure 3.5(c) in Kouyama et al., 2021), leading to the concern that the optical performance may further degrade over the next 10 years.

Kouyama et al. (2021) obtained a degradation trend coefficient of d_TD2 = -0.000252 day–1 from the sensitivity time variation of ONC-T by using observations of stars made during the second touchdown (TD2) between July 2019 and May 2020, assuming a linear degradation progression. However, if the sensitivity of ONC-T continues to degrade linearly with time, it will reach zero at around 4000 days (approx. 11 years) after TD2. Since this “zero-sensitivity” timing would be just before the arrival at asteroid 1998 KY26 in 2031, the sensitivity degradation trend of ONC-T poses a serious problem. The main cause of sensitivity degradation is thought to be the adhesion of asteroid dust to the ONC-T optical system during TD. The mechanism behind the subsequent sensitivity reduction that has continuously occurred since then is not understood, so making a reliable prediction of sensitivity degradation has been difficult. Thus, empirical extrapolation based on actual sensitivity is the only way to make this prediction; we continued to monitor the degradation in ONC-T sensitivity after departing asteroid Ryugu.

To predict whether the sensitivity at the time of flyby and during arrival at the target asteroids will be high enough to conduct the observations necessary for achieving the mission goals of the extended mission, we estimate the sensitivity change using the calibration observation data taken with the flat-field (FF) lamps onboard ONC-T, and stellar observations accumulated from launch until May 2022, which is nearly 3 years after TD2. The extended period for the post-TD health check is much longer than a year, which our previous study (Kouyama et al., 2021) was based on, so we expected to be able to obtain a significantly more reliable prediction of the optical degradation trend now. If the predicted sensitivity at the time of flyby and arrival is high enough, then it will be needed for determining the optimal exposure time for observing the new target asteroids. The objective is also to present updated information on sensitivity changes that will be necessary for future data archiving and reduction. Although detailed calibration of ONC-W1 and W2 has not been performed during cruising after the departure from Ryugu, we took a number of images using both W1 and W2 during the capsule delivery operation. The current status of ONC-W1 and W2 is inferred based on these images.

Sensitivity change of ONC-T
In the following section, we present a comparison among three independent results obtained from FF-lamp observations, stellar observations, and post-Earth swing-by lunar observations, as well as analyses of the sensitivity degradation of ONC and related phenomena. These three methods have their own pros and cons but are highly complementary to each other. Since the FF-lamp observation mode allows for a single light source to illuminate the entire field of view, it is easy to compare sensitivity over time. It is necessary, however, to take into account temperature changes and degradation of the lamp itself. In contrast, stellar observations are suitable for determining absolute sensitivity over time, but measurements can be made for an only limited number of pixels, and opportunities to observe the same star are limited. Lunar observations have an advantage over the other two observation methods in that they provide an unchangeable and extended light source. Thus, the Moon can provide absolute brightness over many more pixels in the CCD than stellar observations without affecting its temporal change. However, this calibration requires comparison with a lunar brightness model, which is much more complex than standard star data and has room for improvements.

Sensitivity variation of ONC-T observed with the FF lamp
The FF lamp is mounted in front of the optical system of the ONC-T and allows almost constant light to enter the photosensitive area of the CCD sensor, even in deep space. This health-check imaging with the FF lamp has been consistently performed with exactly the same sequence and exposure time as imaging during the ground test and cruising. Table 1 summarizes the exposure times and FF-lamp voltage settings for the health-check imaging for each band. By comparing the imaging data with this lamp turned on, we can estimate the sensitivity change of the entire CCD. Figure 1 shows the v-band FF-lamp image acquired in December 2014 immediately after launch. Since the two lamps are installed diagonally, there are two areas that are brighter than the others in the field of view of ONC-T.

The FF-lamp voltage can be set to High or Low, which can be used for short wavelengths (ul (0.4 µm), b (0.48 µm), v (0.55 µm), and Na (0.59 µm) bands) and long wavelengths (w (0.70 µm), x (0.86 µm), p (0.95 µm), and wide bands), respectively. FF lamps at the High voltage setting are too bright for the w, x, and p bands, causing saturation, and those at the Low voltage setting are too dark for ul, b, v, and Na, leading to signal-to-noise ratios that are too low. As discussed by Kameda et al. (2017) and Tatsumi et al. (2019), the bias level, which is the offset of the signal of the ONC CCD, depends on the temperatures of the CCD, the electronic substrate of the camera head, and the ONC analog electric unit (ONC-AE). This temperature dependence of the bias level can be approximately compensated for by smear correction, which subtracts data taken at the minimum exposure time (0 s). The dark current noise caused by thermionic electrons, which depends highly on the CCD temperature, was reduced by using images acquired at low CCD temperatures of below -25 °C. Images with strong “radiator stray light”, whose intensities change greatly as a function of spacecraft attitude (Suzuki et al., 2018; Tatsumi et al., 2019), were not used for calibration analysis. At the Low voltage setting, FF-lamp brightness depends linearly on the temperature of the ONC-AE, as reported by Kouyama et al. (2021). The ONC-AE temperature was not constant during the FF-lamp observations because the ONC-AE was under a passive thermal control that depends on the temperature of the spacecraft. Thus, we linearly corrected the observed brightness to compensate for the effect of AE temperature deviation at -6.8 °C, which was the ONC-AE temperature during the first FF-lamp observation conducted immediately after launch.
Figure 2 shows the change in the sensitivity of the ONC-T determined using FF-lamp images acquired from launch to July 2021. The value on the vertical axis is the average of the count values in all pixels of the CCD divided by the value immediately after launch. FF-lamp images taken around a year after launch indicate that the ul band signal experienced a large (approx. 5%) drop. Subsequently, there was less than a 2% change at most in all bands until arrival at Ryugu in June 2018. There was a 4-5% drop after the first touchdown (TD1) in February 2019, and a 6-7% drop after TD2 in July 2019. These post-TD decreases appear to be greater for shorter wavelength bands. After departure from Ryugu in November 2019, there was no significant decrease, and there may even be a small increase.

Health-check observations using FF lamps after TD operations also showed that ONC-T had some change in lens contamination that we had not seen before. Figure 3a shows an image of the FF lamp acquired prior to the departure from Ryugu in November 2019. This image is not significantly different from the one taken immediately after launch (Figure 1). The next FF-lamp image acquired in February 2020 (Figure 3b) did not have any differences either. In the image taken in September 2020 (Figure 3c), however, dark areas appeared near the center and lower right of the field of view. Subsequently in December 2020, these dark areas were no longer visible in the FF-lamp image after the return to Earth (Figure 3d). Figure 4 emphasizes these dark areas by taking the ratio of the September 2020 FF-lamp image to that taken in November 2019. This black area was about 5% lower than normal. Since these dark areas appeared in all bands of the image, it is suspected that something other than the filter was deposited either on the optics or on the surface of the CCD sensor. This was the first time such a change had appeared in the FF-lamp image since the launch of Hayabusa2 in 2014.

Figures 5 and 6 show the temperature histories of the CCD sensor and the ONC-T optics before and after these dark areas appeared. The CCD sensor is cooled by a radiator that keeps its temperature low (-20 °C or lower) except in special cases. There is no significant difference in the CCD temperature before and after the dark areas appeared. On the other hand, the optical system of the ONC-T fluctuates between low temperatures (approx. -20 °C), which might lead to volatile condensation, during the storage mode and high temperatures (approx. +20 °C), which might lead to evaporation, during the imaging mode. The temperature of the optical system was kept at -20 °C for around 5 months until just before imaging in September 2020, when the dark areas were observed. It was then kept at higher temperatures (approx. +20 °C) until the next FF-lamp imaging 3 months later.

Although the optics had been kept at low temperatures for more than five months during the period between launch and asteroid departure, these dark areas never appeared. The fact that they appeared when the optical system was kept at low temperatures for a long period of time after departing Ryugu suggests that outgas released from asteroid-derived materials adhered to the ONC-T and its surroundings during TD. No such spots appeared in the FF-lamp images taken after the Earth departure until July 2021. Even if similar dark areas appear again, they will likely be eliminated by warming up the optical system and will not interfere with future observations.

Sensitivity variations of ONC-T bands based on stellar observations
Our previous efforts focused on evaluating the absolute sensitivities of ONC-T bands (Tatsumi et al., 2019) and variations in the color sensitivities relative to the v band (0.55 µm) (Kouayama et al., 2021) based on stellar observations. In line with this work, we have added more stellar observations to monitor the sensitivities of ONC-T bands (Figure 7) after the capsule re-entry operation on December 5, 2020. The list of stellar observations is summarized in Table 2. As reported in Kouyama et al. (2021), a 15% degradation in absolute sensitivity had been confirmed in the stellar observations after departure by comparing them to the sensitivity before arrival. On the other hand, only a small variation (up to 2%) in the v-band normalized sensitivity (i.e., sensitivity for the color ratio) was confirmed for any band during the TD operations of Hayabusa2, and the stability of the color ratio had been confirmed in the period during the return phase.

These trends were also confirmed from observations of β Sco and σ Sgr, both of which were observed before TD1 and after departure from Ryugu (Figure 8). In them, we can ignore the uncertainty in the reference spectra used for measuring sensitivity degradation by comparing observations of the same stellar brightness over different days. For the ul, b, and v bands, the degradation was stable and evaluated to be 15.8 ± 0.4 %, 15.3 ± 0.3 %, and 15.8 ± 0.3 %, respectively. The error ranges were evaluated from standard deviations of measured sensitivity degradations in Figure 8. For the bands at longer wavelengths, the degradation was also 15 – 16%, but there were greater fluctuations (approx. 1.5% for Na, w, and x, and 4% for p) in the measurements. We could only obtain calibration observations for ε Aqr before and after TD1, and we could only evaluate the effect of TD1 using this star. However, the observation that the sensitivities of all seven bands are similar to each other is also found in the pre-TD1/post-TD1 comparison. Careful monitoring for possible sensitivity variations in those bands should be required in future work.
It should be noted that after the TD2 operation, the measured sensitives from stellar observations showed a gradual decreasing trend corresponding to 2.5% per 100 days, which continued after departure from Ryugu. Kouyama et al. (2021) concluded that it was difficult to judge whether the degradation trend converged because of the insufficient number of stellar observations. With added stellar observations, however, we can conclude that the sensitivity degradation in ONC-T likely reached the convergence state for all bands in May 2020, which was before the capsule re-entry operation. The magnitude of the degradation at the convergence state was almost 15% for all bands. The updated sensitivity correction coefficients are summarized in Table 3.

Sensitivity variations of ONC-T bands based on lunar observations
Figures 9 and 10 show observed lunar irradiance by ONC-T bands at 08:05 a.m. on December 6, 2020 and modeled irradiance estimated from a lunar reflectance model based on SELENE/SP observations (SP model) (Yokota et al., 2011). Similar to the lunar observations in 2015 (Suzuki et al., 2018), the band ratios between the observations and the model are well consistent, within 5%.

Since the brightness of the Moon has been well studied and modeled (cf. Kieffer and Stone, 2005; Kouyama et al., 2016), the sensitivity of a sensor can be evaluated through a comparison between observed and modeled Moon brightness, which is called a lunar calibration. While the uncertainty in absolute accuracy from the lunar calibration is still under discussion (larger than 5%), the uncertainty for evaluating the relative variation in sensor sensitivity between different wavelength bands is sufficiently small (less than 1%).
In Figure 11a, the ratios of observed and modeled lunar brightness in 2015 and 2020 are plotted for the v, Na, w, x, and p bands. Compared to the results from 2015, those from 2020 indicate clear sensitivity degradation in all bands. 
Figure 11b shows quantitative evaluations of the sensitivity degradation between 2015 and 2020. The results indicate a 10% degradation for all bands. The 10% degradation from the lunar calibration is somewhat smaller than degradation estimations from the stellar and Ryugu observations (approx. 15%; Figure 8) (Kouyama et al., 2021). This approximately 5% discrepancy in sensitivity degradation is consistent with the uncertainty in the accuracy of the lunar calibration. The inconsistencies among different calibration sources should be studied in future work.


Low stray light attitude and noise evaluation in extended missions
To expand the range of possible targets for ONC-T observations, such as to zodiacal light observations and observations of transiting exoplanets, before arrival at the next asteroid in the extended mission, a method for reducing stray light was investigated. It was reported in Suzuki et al. (2018) and Tatsumi et al. (2019) that sunlight reaches the CCD through a small gap near the ONC-T radiator when the spacecraft is oriented in attitudes that allow sunlight to be incident on it. The ONC radiator is mounted on the -Y panel of the spacecraft and is also close to the +X side. Therefore, if the spacecraft is oriented so that the Sun shines on the -X and +Y sides of the spacecraft, then sunlight will not shine directly on the radiator.

Until the capsule was released to Earth in December 2020, the spacecraft was operated in such a way that the -X side of it was not exposed to sunlight. This was done to protect the capsule, which was placed on that side. This restriction was removed after capsule separation. The “stray light from the ONC-T radiator" should be reduced by keeping the Sun on the -X and +Y sides of the spacecraft.
Figure 12 shows the ONC-T stray light intensity (log[DN/s], where DN is the digital number) for the spacecraft attitude from the arrival in June 2018 to departure in December 2020, using the same method as Tatsumi et al. (2019). Observations indicated by the gray circles were taken with long exposures of 100 s or more. The amount of stray light is small in the region where sunlight is incident on the spacecraft’s -X panel (XPNL < 0) and +Y panel (YPNL > 0).

After capsule separation on December 5, 2020, we attempted observations with long exposures of more than 100 s with the Sun on the -X side of the spacecraft, and we confirmed that the signal due to stray light or noise was less than 0.2 DN/s. According to Kameda et al. (2017), the dark current noise of ONC-T at a CCD temperature of -20 °C is approximately 0.1 DN/s, and the <0.2 DN/s result obtained in this trial is comparable to this value. The maximum exposure time of the ONC-T is about 178 s, and even for a target with a very small signal, if 36 counts or more can be expected in that time, then it is possible to image with a signal-to-noise ratio of 1 or better.


Prediction of the sensitivity change and exposure time for the extended mission

A comparison of ONC-T sensitivity changes for the FF lamp and stellar observations shows good agreement, except that no stellar observations were made immediately after launch. Thus, the rapid initial decrease in the ul band observed in the FF-lamp observation cannot be supported with stellar observation. In both observation results, no significant decrease in sensitivity occurred after the return to Earth (capsule re-entry) in December 2020.

We made simple models for predicting future changes in the sensitivity of ONC-T, whose purpose is to evaluate the feasibility of observing the asteroids 2001 CC21 and 1998 KY26 during the extended mission. Figure 13 shows two potential cases for the sensitivity change (Table 3) of the v band that are obtained from stellar observations: (1) no sensitivity decrease and, as the worst case, (2) a decrease rate of 2%/1302 days seen in the early days of FF-lamp observations. In the first case, the relative sensitivity remains 84.1% after April 15, 2020. In the other case, the relative sensitivities during the approach of asteroids 2001 CC21 and 1998 KY26 are estimated to be 80.6% and 77.8%, respectively.

The brightness and albedo of asteroids 2001 CC21 (Binzel et al., 2004) and 1998 KY26 (Ostro et al., 1999) have been reported, but the albedo values of them are highly uncertain at this time. Here, we consider a range of albedo values for the target asteroids with a lower limit of 4%, the same as Ryugu, and an upper limit of 20%. The brightness of asteroids 2001 CC21 and 1998 KY26 was compared to that of Ryugu, taking into account the distance between the asteroids and the Sun. This brightness ratio is, in other words, the ratio of the exposure time required to image Ryugu with ONC-T to the exposure time required to image the asteroids 2001 CC21 and 1998 KY26 (Table 4). 2001 CC21 requires a shorter exposure time than Ryugu due to its smaller solar distance, while 1998 KY26 requires a longer exposure time owing to its larger solar distance. Exposure times for imaging Ryugu ranged from 65 – 131 ms in the v band. By multiplying this range of exposure times by the exposure time ratios in Table 4, we can estimate that asteroid 2001 CC21 can be imaged with exposure times ranging from 11–110 ms, and asteroid 1998 KY26 with exposure times ranging from 22–219 ms. These ranges are within the range of the possible ONC-T exposure time settings. With the exception of the wide band, all bands were within the settable exposure time range, and it was confirmed that ONC-T could observe asteroids 2001 CC21 and 1998 KY26. The wide band used for Ryugu imaging had an exposure time of 8 ms, two steps higher than the minimum settable setting, so the exposure time could not be set sufficiently short to cope with the high albedo of 2001 CC21, indicating that the signal would saturate.

ONC-W1 and W2 sensitivities since departure from Ryugu.
The ONC onboard Hayabusa2 has two wide-angle cameras, W1 (nadir view) and W2 (oblique view) (Suzuki et al., 2018). These cameras do not have FF lamps or high enough sensitives to observe most stars, so we did not have a chance to perform a quantitative health check after the departure from Ryugu. Thus, the Earth return was one of the few opportunities to examine the health of W1 and W2. Furthermore, since the spacecraft reached very close to Earth (approx. 300 km from the surface) when the capsule re-entered the atmosphere, this provided a unique opportunity for observing a fast-moving object relative to the spacecraft. In this section, we discuss the results of the Earth observations and infer the health conditions of the cameras. 

 Status of ONC-W1
Earth imaging using ONC-W1 was successfully performed during the return to Earth in December 2020. The exposure time used was 8.2 ms, which is the same as that used in 2015. While the counts of the oceans in 2015 were about 500 to 600, those in 2020 were about 300 to 400. This level (approx. 60%) of sensitivity degradation is approximately the same as that reported in Kouyama et al. (2021).

ONC-W1 was designed to capture Ryugu images with approximately the same exposure time as the ONC-T. On the other hand, ONC-W1 was also designed to enable target marker imaging using the flash lamp during TD, which was expected to be much brighter than Ryugu. To cover both requirements, ONC-W1 has shorter minimum (170 μs) and maximum (5.6 s) exposure times than those for ONC-T. If ONC-W1 had no sensitivity degradation, then stars brighter than magnitude 1.2 could be observed with the maximum exposure time. 
Jupiter observations in April 2020, which was brighter than a visual magnitude of 0, produced a bright image of Jupiter that was clearly confirmed in the W1 image. Observations of Formalhaut (visual magnitude of 1.2) in May 2022, however, produced no stellar image because it was just at the limiting magnitude. The sensitivity of ONC-W1 should be monitored periodically until the arrival of the target asteroid in the future by using opportunities when brighter stars are observable and when the spacecraft performs another flyby of Earth.

Status of ONC-W2
ONC-W2 was designed to image Ryugu with about 1/6 the exposure time of ONC-T. The maximum exposure time for ONC-W2 was 45 s. If ONC-W2 had no sensitivity degradation, then stars brighter than magnitude 4.6 could be observed with the maximum exposure time. During the return phase, ONC-W2 observed Vega with the maximum exposure time on February 28, 2020. Vega was successfully captured with sufficient DN (approx. 1200 DN, or a signal-to-noise [S/N] ratio of 200), although its position in the ONC-W2 field of view (FOV) was far from center, and it was hard to quantitatively evaluate its sensitivity variation due to uncertainty in the flat field correction for such a region. The sensitivity of ONC-W2 was approximately 3.8 × 103 (DN/s)/(W/m2/sr/μm) (Tatsumi et al., 2019).

 The boresight direction of ONC-W2 is tilted approximately 60 degrees from that of ONC-T. The unique installation angle of this camera was used to attempt imaging of Earth and the capsule during the Earth swing-by on December 6, 2020. Continuous imaging with 1-s exposures was performed, but the capsule could not be detected (see Appendix for details). On the other hand, it successfully observed the city lights of Adelaide and cloud-like patterns over Australia (Figure 14). These results indicate that W2 is still functional and has not experienced sever deterioration in sensitivity.


Conclusion
The data obtained after departure from asteroid Ryugu suggest that ONC-T optical sensitivity degradation may have settled down. Although continued calibration activities are necessary for performing an accurate prediction of sensitivity change, the data we have obtained so far indicate a long-term linear sensitivity change. This suggests that the ONC-T sensitivity should be between 80.6% and 84.1% during the 2001 CC21 flyby and 77.8% and 84.1% during the 1998 KY26 flyby, respectively. These sensitivity levels are expected to be sufficient for performing the necessary observations of these asteroids. 

During the cruise preceding Hayabusa2’s arrival at the target asteroids in the extended mission, opportunities for ecliptic light observations and exoplanet observations can be increased by reducing noise from attitudes in which the Sun shines on the -X and +Y panels of the spacecraft.

Appendix A. Observation with ONC-W2 during the re-entry phase of the return capsule

Since ONC-W2 was rarely used during the return cruise, even during the proximity phase after TD2, it has not been confirmed that any significant optical degradation occurred. We attempted to use the unique installation angle of this camera to image Earth and the capsule during the Earth swing-by operation. We decided to include it in this study as part of a qualitative optical degradation assessment.
Based on the observational result of the maximum brightness of Hayabusa’s return capsule during the re-entry phase of its 2010 mission, the maximum temperature of the return capsule was expected to be around 3000 °C from considerations of blackbody emission, and the altitude during maximum brightness was 55 – 60 km (Sato et al., 2012). We assumed that the return capsule of Hayabusa2 would also use the brightness at 55 – 60 km to determine its temperature. The estimated distance between the capsule and the Hayabusa2 spacecraft would be around 350–400 km at the time of maximum brightness.
Although the size of the capsule (40 cm diameter) was much smaller than the corresponding spatial scale of a ONC-W2 pixel (400 m), even from the minimum distance of 350 km, we confirmed that the capsule would be bright enough to be observed (i.e., the S/N ratio would be 10) within the possible exposure times, assuming a 3,000 °C capsule temperature (Figure A.1). If W2 observes the capsule from a distance of 350 km, then 1 s of exposure would be enough for unambiguous detection if the object were moving with respect to Hayabusa2.
However, it was also expected that the motion of the capsule in the W2 FOV would be approximately 10 pixels within the 1-s exposure owing to the velocity difference between Hayabusa2 and the capsule. Therefore, an effective exposure time for the capsule observation would be 0.1 s, and the possible S/N ratio would be around 5. Although the expected S/N ratio could be marginal, we conducted observations using 1-s exposures with an interval of 2 s during the re-entry phase of the return capsule.
Figure A.2a shows an example of the images obtained on December 5, 2020 during this phase. Since there were clear periodic noise patterns (due to electromagnetic noise), we performed Fourier analysis for each image (Figure A.2b) and reduced the noise by subtracting the top-10 Fourier components for each line, thus enhancing their visibility (Figure A.2c). The formula for doing this can be given by



where aj indicates the amplitude of the j-th largest Fourier component, and bj and fj are its phase and wavenumber, respectively.

Figure A.3 shows a close-up image that includes the region where the capsule was expected to be observed. In this region, there was no clear bright spot that exceeded a S/N level of 3 or 5, compared with the surrounding region. The standard deviation of counts in the image was 1.7 DN; the S/N levels of 3 and 5 corresponded to 5.1 DN and 8.5 DN, respectively.

It is difficult to discuss the implications of an observation result in which no significant signal was detected. However, the unique nature of this particular observation allows us to infer the significance of the fact that ONC-W2 did not detect light from the aerodynamically heated side of the capsule. From the sensitivity and spectral response performance of ONC-W2 (Suzuki et al., 2019; Kouyama et al., 2021), the brightness temperatures that provide 5.1 DN and 8.5 DN for ONC-W2 from a 350 km distance are 2,125 K and 2,224 K, respectively (Figure A.4). This means that the apparent brightness temperature from ONC-W2 might not reach 3,000 °C.

It should be noted from the investigation of the return capsule of the first mission that the back side of the capsule experienced only approximately 650 K heating (Sato et al., 2012), while the front side of the capsule experienced 3,000 °C. Therefore, if ONC-W2 observed both the front and back sides of the capsule, then the apparent brightness of it should be much darker than the brightness for 3,000 °C.
Figure A.5 shows a schematic view of a geometric configuration for the capsule observation by ONC-W2 based on the planned trajectories of the capsule and Hayabusa2 during the re-entry phase. Assuming the shape of the capsule to be a sphere for simplicity, the front side of it (higher temperature) occupies only 6.7% of the capsule’s silhouette seen from ONC-W2. In this case, the apparent brightness of the capsule corresponds to 2,150 K, even if the front side of the capsule reached 3,000 °C. A temperature of 2,150 K is almost the same as that for a S/N level of 3, and thus, the geometric configuration and relatively low temperature of the capsule’s backside can be reasons why ONC-W2 could not capture a clear signal from the capsule.

It has been noted that post-flight analysis of the onboard accelerometers indicates that the attitude of the return capsule was very stable at high altitudes, where high aerodynamic heating took place. A large-amplitude rotation only took place at low altitudes ≲ 20 km (Yamada and Yoshihara, 2022). This is consistent with our result that ONC-W2 did not detect significant light during the atmospheric re-entry of the capsule.
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Figure legends

Figure 1. FF-lamp image taken with the ONC-T v band in December 2014.

Figure 2. History of ONC-T sensitivity changes from launch to July 2021.

Figure 3. ONC-T v-band FF-lamp images acquired from just before departure from Ryugu (November 3, 2019) to after capsule re-entry (December 28, 2020). Dark areas only appeared on September 30, 2020 near the center and lower right of the image.

Figure 4. The dark areas are emphasized by taking the ratio of the FF-lamp image taken on September 30, 2020, in which the dark areas appeared, and the FF-lamp image taken on November 3, 2019, which was acquired just before departure from Ryugu.

Figure 5. Optics temperature history for ONC-T from November 2019 to July 2021.

Figure 6. History of the CCD sensor temperature for ONC-T from November 2019 to July 2021.

Figure 7. Sensitivity variations of the ul – x bands measured from stellar observations since Hayabusa2’s launch. The measured sensitivity for each band was normalized by the value in Tatsumi et al. (2019), which was measured in space before arrival. A fitted trend for the sensitivity degradation of the v band after TD2 is also plotted (dotted line).

Figure 8. Sensitivity variations of the ONC-T bands measured from specific stars that were observed more than two times.

Figure 9. (a) A lunar image obtained by ONC-T (v band) on December 6, 2020, and (b) a simulated image calculated by the SP model (Yokota et al., 2011).

Figure 10. Observed lunar irradiance taken at 2020-12-06 08:05 (dots) and the modeled spectrum (solid line).

Figure 11. (a) Ratios between the observed and modeled lunar brightness. The model brightness was estimated based on the SP model. (b) Sensitivity degradation between 2015 and 2020 for the lunar observations evaluated in (a).

Figure 12. Stray light intensity of ONC-T for spacecraft attitudes taken from June 27, 2019 to December 26, 2020. Gray circles show observations made with a long exposure (>100 s).

Figure 13. Model of sensitivity changes for ONC-T in the v band. Changes up to April 15, 2020 are from stellar observations (Table 3). After that, the red line shows the case with a sensitivity decrease, and the green line shows the case with no change.

Figure 14. a) Australia imaged by ONC-W2 at 02:29 a.m. on December 6, 2020 (two minutes before closest approach to Earth). The bright spot on the left of the image comes from the city lights of Adelaide. b) Simulated night view of an ONC-W2 image at the same time. c) Simulated image with the topography visible.



Figure A.1　Required exposure times for observing the return capsule with a S/N ratio of 10 as a function of observation distance. A gray line indicates the maximum exposure time of ONC-W2 (44 s), and the hatched region indicates conditions in which ONC-W2 is capable of observing the capsule.

Figure A.2 (a) An example of an ONC-W2 image when the capsule is expected to have maximum thermal emission. (b) A synthetic image generated from the top-10 Fourier components in (a). (c) A noise reduced image derived from (a) and (b).

Figure A.3 A close-up of an ONC-W2 image that includes the expected region where the return capsule was observed (indicated by a dotted rectangle), taken at 17:29:02 p.m. on December 5, 2022.

Figure A.4. Relationship between the apparent brightness temperature and the DNs of ONC-W2, observed from a 350 km distance.

Figure A.5 A schematic view of the capsule observation geometry for ONC-W2 at the time of maximum brightness, based on the planned trajectory information for the capsule and Hayabusa2.


Table legends

Table 1. Settings for performing health-check imaging with the FF lamp.

	Bands
	Center wavelengths  [nm]
	Bandwidth [nm]
	Exposure times for FF-lamp imaging [ms] 
	FF-lamp settings 

	ul
	390.4 
	45
	1049
	HIGH

	b
	479.7 
	25
	524.8
	HIGH

	v
	549.0 
	28
	131.2
	HIGH

	Na
	590.1 
	10
	174.1
	HIGH

	w
	700.4 
	28
	348.2
	LOW

	x
	858.9 
	42
	65.6
	LOW

	p
	949.7 
	57
	65.6
	LOW

	wide
	775.0 
	850
	5.44
	LOW










Table 2. List of stars used in Figure 7. Note that ε Aqr, β Sco, and σ Sgr were observed two times, three times, and four times, respectively.
	Observation date
	Star name
	HR no.
	V mag
	Spectral type
	Filters
	Reference spectra

	2016-10-19
	ζ Peg
	8634
	3.40
	B8V
	ul, b, v, Na, w, x, p
	Hamuy et al. (1992, 1994)

	2017-05-23
	θ Crt
	4468
	4.70
	B9.5Vn
	ul, b, v, Na, w, x, p
	Hamuy et al. (1992, 1994)

	2017-10-10
	ε Aqr
	7950
	3.77
	A1V
	ul, b, v, Na, w, x, p
	Hamuy et al. (1992, 1994)

	2017-10-12
	σ Sgr
	7172
	2.02
	B2.5V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	Arrival (2018-06-27)

	2018-08-25
	β Vir
	4540
	3.60
	F9V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2018-11-09
	β Sco
	5984
	2.62
	B1V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	TD1 (2019-02-21)

	2019-03-09
	ε Aqr
	7950
	3.77
	A1V
	ul, b, v, Na, w, x, p
	Hamuy et al. (1992, 1994)

	TD2 (2019-07-11)

	2019-07-14
	ι Aur
	1577
	2.69
	K3II
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2019-07-18
	β Tau
	1791
	1.65
	B7III
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2019-09-26
	η Leo
	3975
	3.45
	A0Ib
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2019-11-03
	γ Crv
	4662
	2.56
	B8III
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	Departure (2019-11-13)

	2020-03-15
	τ Sco
	6165
	2.82
	B0.2V
	ul, b, v, Na, w
	Alekseeva et al. (1996)

	2020-05-04
	σ Sgr
	7172
	2.02
	B2.5V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	Capsule re-entry operation (2020-12-05)

	2020-12-19
	κ Ori
	2004
	2.06
	B0.5Ia
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2021-04-16
	β Sco
	5984
	2.62
	B1V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2021-05-17
	σ Sgr
	7172
	2.02
	B2.5V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2022-01-19
	β Vir
	4540
	3.60
	F9V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2022-03-03
	β Sco
	5984
	2.62
	B1V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)

	2022-04-11
	σ Sgr
	7172
	2.02
	B2.5V
	ul, b, v, Na, w, x, p
	Alekseeva et al. (1996)



Table 3. Sensitivity factors at the reference temperature (TCCD, T = -30 °C), and errors for the band ratios from stellar observations.
	Sensitivity (DN/s)/(W/m2/µm/sr) at TCCD, T = -30 °C

	
	Filters
	ul
	b
	v
	Na
	w
	x
	P

	Before TD1a
	Sensitivity
	439.1 ± 2.2
	969± 7.9
	1175.0 ± 10.0
	546.9 ±2.0
	1515.0 ± 19.3
	1499.8 ± 24.6
	961.2 ± 28.8 b

	After TD1
	Sensitivity
	410.1 ± 11.6
	899.1± 22.2
	1092.8 ± 25.5
	510.9 ± 12.2
	1418.9 ± 35.1
	1405.8 ± 40.7
	898.9 ± 39.8

	After TD2
	Degradation trend
	-0.000252 day-1

	
	Sensitivity at TD2
	399.7 ± 10.8
	879.6 ± 22.1
	1071.2 ± 25.0
	498.3 ± 11.9
	1380.5 ± 34.0
	1373.5 ± 37.4
	882.6 ± 38.9

	After capsule re-entry
	Sensitivity
	363.3 ± 9.0
	810.2 ± 16.1
	988.5 ± 10.3
	469.5 ± 6.7
	1279.4 ± 21.8
	1276.7 ± 38.2
	806.2 ± 30.1 c


aTatsumi et al. (2019). b Value based on lunar observations. c Value from observing the same star at different times.

Table 4. Estimated relative sensitivities and exposure time ratios for the new target asteroids.
	Asteroid
	Ryugu
	2001 CC21
	1998 KY26

	Spectral types
	C

	L

	L


	Arrival date *
	2018/06/27
	2026/07/15
	2031/07/15

	Days since arrival at Ryugu
	0

	2940

	4766


	Estimated relative sensitivity [%]
	---


	80.6 - 84.1


	77.8 - 84.1



	Heliocentric distance [km]
	1.4665E+08

	1.2062E+08

	1.6710E+08


	Albedo [%]
	4
	20
	4
	20
	4

	Exposure time ratio **
	1

	0.17

	0.84

	0.33

	1.67



* Because the exact arrival date has not yet been determined, we chose a date near the middle of the expected arrival month.
** Value for the worst expected sensitivity.
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