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a: the Pb concentration value indicated in the BCR-032 is an estimated value and not a certified value. b: the Co concentration value indicated in the BCR-414 is an estimated value and not a certified value. DLs: Detection limits. RSD: Relative Standard Deviation.
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  BCR - 032  BCR - 414  

Element  DLs   (µg/L)  Certified value  (mg   /Kg)  Mesured value  (mg/Kg)  RSD  (%)  Rec  (%)  Certified value  (mg /Kg)  Mesured value  (mg/Kg)  RSD  (%)  Rec  (%)  

Cd  0.1  20.80  21.2  1.54  101.90  0.383  0.396  2.1  103.39  

Co  0.2  0.59  0.54  2.5  91.50  1.43   b  1.52  0.34  106.29  

Cu  0.4  33.70  32.90  0.32  97.60  29.5  31.2  0.31  105.76  

Cr  0.2  257  255.30  2.9  99.30  23.8  22.6  0.21  94.96  

Ni  0.5  34.60  32.70  0.47  94.50  18.8  17.5  0.22  93.08  

Pb  1  5.40  a  5.36  2.5  99.30  3.97  3.72  0.16  93.07  

Zn  0.2  253  2.49  4.9  98.40  111.6  112.4  3.2  100.72  

 


