Highlights	

· [bookmark: _GoBack]Bayesian Model Averaging (BMA) technique was applied to combine forecasts from evaporation estimation methods and analysis of their uncertainty for the first time.
· BMA and Hamon methods performed better than the rest of the models in terms of the accuracy of evaporation estimation
· BMA significantly reduced uncertainty associated with the estimation of evaporation in all months
· Applying different evaporation methods influenced the resilience index and vulnerability index of the reservoir



