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Fig. ES1 TEM images of prepared organophilic clays 








2.Scanning electron microscopy analysis
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Fig. ES2 SEM images of prepared organophilic clays 
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