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Fig. S1 The optical images of the sol-gel coatings with different ratios: (a) A31, (b) A21, (c) A52, (d) A41 and (e) A24 (The scale bars are 200 μm)
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Fig. S2 The optical micrographs of cross cut adhesion test on sol-gel nanohybrid coatings on PC: (a) 4PA24 and (b) 6PA12
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Fig. S3 The optical micrographs of pencil impressions on: (a) bare PC by 4B pencil and (b) on 4PA24 coating by 3H pencil
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Fig. S4 The optical micrographs of pencil scratch impression with different scale bars: (a,b) 200 μm and (c,d) 100 μm
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