


Highlights:
· A progressive forming system directly using continuous metal wires was developed.
· [bookmark: OLE_LINK11]Meso-/micro-scaled fork-shaped parts with various grain sizes were fabricated.
· Material flow behavior of specimens was found to be related to specimen size.
· Springback-induced dimensional errors were found to increase with grain size.
· Specimen and grain size effects present various influences on forming quality.




