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[image: ]Figure S1. PCR regression models for sediment clay and organic matter prediction. The test set method calibration and validation results for both clay and organic matter assessment (a), and the cross-validation method calibration and validation results for both clay and organic matter assessment (b) are presented.
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