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Figure S1. Size distribution of fiber diameter for the samples investigated
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Figure S2. 3D view of AFM images recorded on squared regions (5 µm per side) of the samples
[image: ]
Figure S3. Pore diameter distribution of the membranes tested for vacuum-assisted ultrafiltration.
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