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The optimal casting parameters was found by Taguchi method
Increasing overheating and decreasing speed inhibited clogging 
Increasing overheating and decreasing speed mitigated peeling defects
Strip produced using the optimized parameters fulfilled the requirement
