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Fig. S1. Viscosity measurement of fabricated PVAPh based fibrous mats
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Fig. S2. SEM of fabricated fibrous mats from PVAPh 4% (w/v)
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