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Figure S1. Actual data versus predicted responses for Power density (a), coulombic efficiency (b), azo dye removal (c), COD removal (d)
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Figure S2. Voltage graph obtained from optimum experiment across 100 Ω external resistance (b)
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