Table 1: Recording of drilling data for a 100 mm depth hole
	Time (sec)
	Z-axis
(mm)
	Motion
	
	Time (sec)
	Z-axis
(mm)
	Motion

	0
	+ 2
	
	Rapid at staring position
	
	18
	-85
	
	Return to current depth level

	5
	- 40
	
	Drill depth of Zone 1 (F500, S2000)
	
	19
	-90
	
	4th peck in Zone 3 (F300 S1400)

	6
	- 50
	
	1st peck in Zone 2 (F400 S1800)
	
	19
	-82
	
	Rapid retraction (8 mm)

	6
	- 46
	
	Rapid retraction (4 mm)
	
	20
	-90
	
	Return to current depth level

	7
	- 50
	
	Return to current depth level
	
	20
	-92
	
	1st peck in Zone 4 (F200 S1000)

	9
	- 60
	
	2nd peck in Zone 2 (F400 S1800)
	
	21
	-86
	
	Rapid retraction (8 mm)

	9
	- 56
	
	Rapid retraction (4 mm)
	
	21
	-92
	
	Return to current depth level

	9
	- 60
	
	Return to current depth level
	
	22
	-94
	
	2nd peck in Zone 4 (F200 S1000)

	11
	- 70
	
	3rd  peck in Zone 2 (F400 S1800)
	
	22
	-86
	
	Rapid retraction (8 mm)

	11
	- 66
	
	Rapid retraction (4 mm)
	
	23
	-94
	
	Return to current depth level

	12
	- 70
	
	Return to current depth level
	
	24
	-96
	
	3rd peck in Zone 4 (F200 S1000)

	13
	-75
	
	1st peck in Zone 3 (F300 S1400)
	
	24
	-88
	
	Rapid retraction (8 mm)

	13
	-67
	
	Rapid retraction (8 mm)
	
	25
	-96
	
	Return to current depth level

	14
	-75
	
	Return to current depth level
	
	26
	-98
	
	3rd peck in Zone 4 (F200 S1000)

	15
	-80
	
	2nd peck in Zone 3 (F300 S1400)
	
	26
	-90
	
	Rapid retraction (8 mm)

	15
	-72
	
	Rapid retraction (8 mm)
	
	27
	-98
	
	Return to current depth level

	16
	-80
	
	Return to current depth level
	
	28
	- 100
	
	 Last peck (F200, S1000)

	17
	-85
	
	3rd peck in Zone 3 (F300 S1400)
	
	29
	- 100
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	Dwell 10 seconds

	17
	-77
	
	Rapid retraction (8 mm)
	
	40
	+ 2
	
	Full retraction at starting position
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