Supporting Information
Figure captions
Fig. S1 Catalytic performance of CuMnCeOx/Cordierite catalysts with different calcination temperatures and times
Fig. S2 The repeatability and stability of CuMnCeOx/Cordierite catalysts





























Figures
Fig. S1
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Fig. S2
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