1. The erosion phenomenon and law of the stability region between the d-axis stator voltage and the q-axis stator voltage during full-speed operation of a SHSEAC were studied.
2. A stable migration control optimization method considering the velocity fluctuation process is proposed, and it is verified by experiments that this method can effectively reduce the velocity fluctuation and increase the maximum velocity.
