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Where:
Qf/Qg: ratio of the absorbed mass of toluene per gram of rubber;
z: ratio of load mass per unit mass of rubber;
a: constant angular coefficient of the straight;
b: constant linear coefficient of straight.
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Where:
Q: mass of toluene absorbed per gram of rubber;
Ws: mass of the swollen composite, after equilibrium reached (g);
Wd: dry composite mass (g);
Wr: mass of rubber in the dry composite (g);
Wf: total formulation mass (g);
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