Table 2. Hydraulic conductivity values and main statistical parameters estimated with the time lag and tidal efficiency methods in each monitoring well during three one-week periods.
	Well
	K (m/d)

	
	November 2019
	January 2020
	May 2020

	
	Time lag method
	Tidal efficiency method
	Analytical solution on sloping beaches
	Time lag method
	Tidal efficiency method
	Analytical solution on sloping beaches
	Time lag method
	Tidal efficiency method
	Analytical solution on sloping beaches

	A2
	27.6
	5.53
	7.19
	53.02
	5.08
	8.29
	48.66
	4.83
	9.52

	A4
	38.96
	5.61
	8.44
	55.93
	4.95
	7.46
	45.55
	4.88
	8.12

	A6
	53.93
	6.57
	7.64
	55.97
	5.24
	7.70
	57.03
	5.11
	8.18

	A8
	48.45
	7.05
	7.93
	57.03
	5.58
	5.97
	77.38
	4.49
	6.83

	B2
	36.36
	14.30
	7.68
	70.07
	6.68
	15.64
	77.17
	5.23
	9.30

	B4
	41.84
	17.44
	7.45
	70.11
	8.40
	9.20
	75.30
	3.55
	8.93

	B6
	51.52
	8.82
	5.66
	60.15
	5.85
	7.04
	92.24
	3.26
	6.60

	B8
	53.76
	9.20
	6.16
	103.58
	7.11
	7.34
	92.24
	3.58
	6.22

	C2
	44.93
	6.38
	7.47
	56.01
	3.92
	8.97
	60.62
	4.16
	8.71

	C4
	48.23
	6.89
	7.78
	53.89
	4.36
	9.16
	80.34
	4.11
	9.21

	C8
	51.78
	7.94
	6.52
	62.17
	4.65
	7.75
	83.73
	3.85
	7.66

	
	
	
	
	
	
	
	
	
	

	Range
	26.33
	11.91
	2.78
	50.56
	4.49
	9.60
	46.69
	1.97
	3.30

	G. mean
	44.42
	8.12
	7.22
	63.74
	5.49
	8.38
	69.98
	4.23
	8.04

	Median
	48.23
	7.05
	7.47
	57.03
	5.24
	7.75
	77.17
	4.16
	8.18

	StDa
	7.92
	3.62
	0.79
	14.50
	1.26
	2.39
	15.64
	0.65
	1.10


a StD: standard deviation

