
Table 1. Photos of Residents’ Homes

	[bookmark: _Hlk115538417]A Group
	B Group
	C Group

	Housing group with excellent high-performance windows and insulation
	Housing group with relatively good insulation
	Housing group with 
aged buildings with sub-par insulation
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Table 2. Sensors and Communication Devices Used
	M2 Hub
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	T1 Sensor
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	Smart Plug
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[bookmark: _GoBack]Table 3. Energy use patterns by group in winter
	Devices
 using Energy
	A-Group
	B-Group
	C-Group

	TV
(max: 100Wh)
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	Electric Rice
Cooker
(max: 340Wh)
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	Electric Blanket
(max: 140Wh)
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	x-axis: Time per hour
y-axis: Electricity consumption (y-axis max: 100Wh [TV], 340Wh [Electric Rice Cooker], 140Wh [Electric Blanket])
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