Supplementary figure legends
Supplementary Figure 1. Full width at half maximum method
The border CT density is defined as CT density of half value between the baseline and the peak, and full width at half maximum is defined as the distance between the two border CT density points at both sides.
Supplementary Figure 2. Inflection point method
The estimated calcium thickness by IP was defined as the distance between the rising and falling IP which are derived from differential curve of the CT density profile curve.
IP = inflection point
Supplementary Figure 3. Agreement between estimated calcium thickness, from full width at half maximum and inflection point, and measured calcium thickness in validation dataset
Scatter plots of relationship and Bland–Altman plots of the mean differences between E-Calc-thick from FWHM (A) and IP (B), and M-Calc-thick showed poor agreement.
E-Calc-thick = estimated calcium thickness; FWHM = full width at half maximum; IP = inflection point; M-Calc-thick = measured calcium thickness by optical coherence tomography; SD = standard deviation

