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Fig. S1. 3D surface profiles of HCFs (P1-HCF).
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Fig. S2. Reliability test of the pressure sensor device.
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Fig. S3 (a, b). Reversibility test experiment of the pressure sensor device.



