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Fig. S1  The ATR-FTIR spectra of NO EF-BC, 1mA-BC, 3 mA-BC, and 5 mA-BC hydrogels.
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Fig. S2  The XRD spectra of NO EF-BC, 1mA-BC, 3 mA-BC, and 5 mA-BC hydrogels 
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