· Electrooxidation integrated membrane bioreactor reduce internal fouling
· Experimental results well fiited with reformulated Hermia model
· Higher rate constant and activation energy obtained through Lumped parameter kinetic modeling
· Thermodynamic parameter exhibits spontaneity and feasiblty of the reaction
