Highlights
· NaA zeolite supported CoxFey with various molar ratio of Fe/Si and Co/Fe was synthesized by a facile hydrothermal process.
· [bookmark: _GoBack]For NaA zeolite supported Co2Fe1/PMS system, 95.8% AO7 and 79.1% COD conversion could be achieved at 20 and 60 min, respectively.
· NaA zeolite supported Co2Fe1/PMS system exhibited excellent catalytic effect and low ions leaching concentration in a wide pH range of 3-9.
· The k values of NaA zeolite supported Co2Fe1/PMS were very high, which were about 16 and 110 times higher than that of pure PMS system at 60 and 50 ℃, respectively.
· The conversion ratio of AO7 still reached 91.8% within 30 min in the third cycle.

