Table 4 Simulation results of CFD
	Parameter
	Direction of rotation
(s=5000rpm; h=0.4mm)
	Rotation speed
(clockwise; h=0.4mm)
	Polishing gap
(clockwise; s=5000rpm)

	Cloud diagram of shear stress  
	Clockwise
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	Counter-clockwise
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	4000rpm
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	5000rpm
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	6000rpm
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	0.2mm
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	0.4mm
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	0.6mm
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	Shear stress of feature point 
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