

Table 3
Thermodynamic parameters for the adsorption of TIB and BTP on mild steel at optimum concentration in 0.5 M HCl at 298 K
	Inhibitor 
	R2
	×10-6 (mol-1)
	 (kJ/mol)

	TIB
	0.982
	0.0102
	45.62

	BTP
	0.941
	0.00261
	39.04




