Table 1. Averaged numbers of counts and the standard deviations (SD) for high tide and low tide and for the 5-min bin width and 2-min bin width.

		Bin width (min)	Averaged number of counts		SD

High tide 	2		               1,525				38.1
Low tide 	2		               1,607				41.3
High tide 	5		               3,807				64.4
Low tide 	5		               4,013				65.5



Table 2. Threshold and the bit error rate respectively chosen and measured in the current work.  

Bin width			5 minutes			2 minutes

Threshold		              3,905			            1,562
Bit error rate		              6%			            16%



Table 3. Results of text message transfer.

MTTI		Transferred text			Time required to transfer

Original	thus air of a double density		-
5 minutes 	ghus air of r noublejdensiwy		700 minutes
2 minutes	jruswkyr nfeagdruklewfeisguq	280 minutes


