Table 2 Classification matrix for spatial and temporal discriminant analysis (HW= Hight Water lever, LW = Low Water lever, IP = Interim Period, T = Total)
	Classification matrix for spatial DA

		Standard mode
	Stepwise mode

	
	% CA
	Center
	Channel
	Mouth
	T
	% CA
	Center
	Channel
	Mouth
	T

	Center
	87.23
	41
	1
	5
	47
	91.49
	43
	1
	3
	47

	Channel
	46.15
	6
	6
	1
	13
	30.77
	9
	4
	0
	13

	Mouth
	51.35
	18
	0
	19
	37
	48,65
	19
	0
	18
	37

	T
	61.58
	65
	7
	25
	97
	56.97
	71
	5
	21
	97




	Classification matrix for temporal DA

		Standard mode
	Stepwise Forward
	Stepwise Backward
	

	
	%CA
	LW
	HW
	IP
	T
	%CA
	LW
	HW
	IP
	Total
	%CA
	LW
	HW
	IP
	T

	LW
	97,14
	34
	0
	1
	35
	97,14
	34
	0
	1
	35
	97,14
	34
	0
	1
	35

	HW
	86,49
	2
	32
	3
	37
	86,49
	2
	32
	3
	37
	86,49
	2
	32
	3
	37

	IP
	44
	4
	10
	11
	25
	36
	4
	12
	9
	25
	44
	4
	10
	11
	25

	T
	75,88
	40
	42
	15
	97
	73,21
	40
	44
	13
	97
	75,88
	40
	42
	15
	97


















Table 3: Classification functions for spatial and temporal discriminant analysis (LW = Low Water level, HW = High Water and IW = Intermediate Period, RW_M = River mouth)
	Spatial variation

		
	Standard mode
	Stepwise mode

	
	Center
	Channel
	Mouth
	Center
	Channel
	Mouth

	Intercept
	-463.819
	-447.792
	-471.573
	-210.280
	-193.418
	-223.695

	Temp
	16.303
	15.665
	16.726
	14.560
	13.842
	14.972

	Sal
	-1.340
	-1.206
	-1.366
	-0.482
	-0.341
	-0.517

	Turb
	0.156
	0.146
	0.175
	0.217
	0.209
	0.237

	pH
	56.983
	56.653
	56.176
	
	
	

	N_NO2
	0.344
	0.354
	0.357
	
	
	

	N_NH4
	0.012
	0.009
	0.018
	-0.021
	-0.026
	-0.016

	NT
	1.942
	2.024
	1.932
	
	
	

	PT
	0.035
	0.041
	0.039
	
	
	

	P_PO4
	0.067
	0.046
	0.056
	
	
	




	Temporal variation

		
	Standard mode
	Stepwise Forward mode
	Stepwise Backward mode

	
	LW
	HW
	IP
	LW
	HW
	IP
	LW
	HW
	IP

	Intercept
	-740.544
	-622.315
	-664.700
	-693.192
	-581.279
	-622.355
	-708.788
	-592.778
	-634.129

	Temp
	28.225
	25.260
	26.693
	26.857
	24.066
	25.454
	27.630
	24.687
	26.110

	Sal
	1.619
	1.029
	1.291
	1.505
	0.917
	1.180
	1.535
	0.948
	1.208

	Turb
	0.223
	0.196
	0.212
	0.276
	0.242
	0.257
	0.203
	0.177
	0.192

	pH
	68.231
	65.958
	65.554
	63.472
	61.213
	60.787
	62.957
	60.872
	60.379

	N_NO2
	0.496
	0.479
	0.487
	
	
	
	
	
	

	N_NH4
	0.125
	0.097
	0.100
	0.094
	0.071
	0.072
	0.110
	0.082
	0.085

	NT
	1.216
	1.145
	1.224
	1.132
	1.074
	1.152
	1.232
	1.159
	1.239

	PT
	0.103
	0.088
	0.090
	
	
	
	0.100
	0.085
	0.087

	P_PO4
	-0.128
	-0.095
	-0.108
	
	
	
	-0.096
	-0.065
	-0.077













Table 4 : Standardized coefficients of the linear discriminant function of spatial and temporal variation (Eig.Val = Eigenvalue, Cum.Eig = Cumulative Eigenvalue.)
	Spatial variation

		
	Standard mode
	Stepwise mode

	
	LD1
	LD2
	LD1
	LD2

	Temp
	0.791
	0.044
	0.843
	0.158

	Sal
	-0.678
	-0.697
	-0.791
	-0.854

	Turb
	0.774
	-0.565
	0.799
	-0.981

	pH
	-0.158
	0.381
	
	

	N_NO2
	0.054
	-0.229
	
	

	N_NH4
	0.316
	-0.189
	0.339
	-0.159

	NT
	-0.155
	-0.202
	
	

	PT
	0.034
	-0.579
	
	

	P_PO4
	0.002
	0.700
	
	

	Eig.Val
	7.246
	3.415
	7.085
	2.468

	Cum.Eig
	0.818
	1.000
	0.892
	1.000




	Temporal variation

		
	Standard mode
	Stepwise Forward mode
	Stepwise Backward mode

	
	LD1
	LD2
	LD1
	LD2
	LD1
	LD2

	Temp
	-1.107
	0.402
	-1.064
	0.468
	-1.108
	0.407

	Sal
	-1.372
	0.127
	-1.416
	0.196
	-1.379
	0.143

	Turb
	-0.332
	0.276
	-0.420
	0.024
	-0.335
	0.284

	pH
	-0.192
	-0.447
	-0.234
	-0.467
	-0.201
	-0.432

	N_NO2
	0.048
	-0.093
	
	
	
	

	N_NH4
	-0.463
	-0.526
	-0.420
	-0.599
	-0.465
	-0.523

	NT
	-0.164
	0.665
	-0.135
	0.777
	-0.166
	0.671

	PT
	-0.225
	-0.422
	
	
	-0.226
	-0.422

	P_PO4
	0.224
	-0.120
	
	
	0.229
	-0.131

	Eig.Val
	20.207
	3.952
	19.755
	3.625
	20.186
	3.936

	Cum.Eig
	0.963
	1.000
	0.967
	1.000
	0.963
	1.000






