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Figure S1. Cross sectional SEM images of Ca-NaNbO3 ceramics with x of (a) 0.05, (b) 0.10, (c) 0.13, (d) 0.15, and (e) 0.20. Composition dependence of average grain size of the samples in Fig. 1(f) was obtained using these SEM images.
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