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Figure S1. HR-TEM and FFT images (right, inset) of pitch-based carbon material (a) P4401-1000, (b) P4401-1300, (c) P4401-2400.




Figure S2. XPS survey scan of pitch-based carbon material.





Figure S3. Nitrogen adsorption-desorption isotherm of pitch-based carbon material.
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