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Fig. S1: Calibration Curve for DMP.



Fig. S2: Adsorption capacities (qt) of DMP by varying the contact time.


Fig. S3: Langmuir fitting curve for DMP adsorption.


Fig. S4: Freundlich fitting curve for DMP adsorption.
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