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[bookmark: _GoBack]Illstration of fabrication and electrochemical characterization of CGC-X as the electrode for double electric layer capacitor.
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Activated at 500°C for 1 h
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Excellent capacitive performance




