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Figure S1. Fourier transform infrared absorption spectra of raw sludge and sludge immobilized chitosan.





Figure S2. Mn concentrations profiles during Mn(VII) biosorption by RCS
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