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Fig. S1 Theory of evanescent around optical fibre for refractive index measurement
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	(a) Schematic diagram of the system
	(b) Cell size and position of the cell when the lid is opened

	

Fig. S2 Measurement system of refractive index during microwave irradiation
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