1) The microstructure and tribological behavior of Ni60 alloy coating were studied.
2) The elements and phase composition of powder and coating are basically the same. 
3) The microhardness and bonding strength of the coating were the highest when the spraying distance is 120 mm.
4) When the friction temperature is higher, the coating wear is more serious.

