Table 1: The milling parameters that were used in this study.
 Milling Process Parameters.
Ball diameter (mm)	                                                           5
Vial Volume (ml)	                                                          100
Ball to powder weight ratio (BPR)	                                  10.1
Ball and vial material	                                                          Stainless Steel
Temperature	                                                                      Ambient

Table 2: The various 3D printing parameters that were followed in this study.
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Variation Details  Nozzle Temperature Bed plate temperature Chamber temperature

(°C) (°C) (°C)
Nozzle t . 160 90
0zzle temperature 160 90

variation

160 90
450 90
Bed plate temperature 450 90
variation 450 90
450 160
Chamber temperature 450 160

variation 450 160




