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Figure F4 – Receiver Operator Characteristic curve of the most discriminating parameters between the CG and smoking patients. Resonance frequency (A) and peripheral resistance (B).
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Receiver Operator Characteristic curve of the most discriminating 


parameters between the CG and 


smoking patients. Resonance frequency (A) and 


peripheral resistance (B).
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A           B    Figure  F 4   –   Receiver Operator Characteristic curve of the most discriminating  parameters between the CG and  smoking patients. Resonance frequency (A) and  peripheral resistance (B).  
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