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Figure F3 – Receiver Operator Characteristic curve of the most discriminating parameters between the CG and PG2–3. Resonance frequency (A) and peripheral resistance (B). 
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A             B    Figure  F 3   –   Receiver Operator Characteristic curve of the most discriminating  parameters between the CG and PG2 – 3 . Resonance frequency (A) and peripheral  resistance (B).     
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