Research highlights

· Cohesiveness and good flowability of the produced powders specifies proper handling properties.

· Spray-drying process is an effective technique for production of spray-dried chlorella peptides. 
· Physicochemical, functional, antioxidant activity and microstructural properties can be maintained using spray drying.

· Combination of maltodextrin, gum arabic, alginate and pectin as carrier effectively used within spray drying.

