Supplementary information

Parameter values of the SRP load model that includes SRP loss due to pH (HP) and that considers the whole basin area as SRP source. * kp is fixed for the model.

	Parameters
	Estimated contribution of source (β)
	In-stream SRP loss process (ks)
	SPR transport from land to water (α)
	SRP loss process depending on pH (kp)

	Units
	kg SRP/km2 yr
	km-1
	yr/m
	km-1

	Mean ± SD
	92.4 ± 7.2 
	0.013 ± 0.013
	8.0 ± 2.9
	0.1*
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