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Supplementary Material


Fig. S1 Phase composition of the brass products used in this work.
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Fig. S2 Elemental maps of the sample surface in Fig. 7a and o of the main text.





Fig. S3 Phase composition analysis of the etched pw-brass samples after immersion in hot water at 75 °C for 45 minutes. PbO was detected on the surface.
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