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Figure S1. Structure of B-BTD-1,4
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Figure S2. Structure of B-BTD-1,3,5
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Figure S3. Structure of B-BTD-1,2,4,5
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Figure S4. Powder X-ray diffraction (PXRD) of the three types of B-BTD-CMPs.
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Figure S5. Solid state 13C CP/MAS NMR spectrum of B-BTD-1,4.
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Figure S6. Solid state 13C CP/MAS NMR spectrum of B-BTD-1,3,5.
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Figure S7. Solid state 13C CP/MAS NMR spectrum of B-BTD-1,2,4,5.
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Figure S8. N2 absorption/desorption isotherms and pore size distribution of the B-BTD-1,4.
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Figure S9. N2 absorption/desorption isotherms and pore size distribution of the B-BTD-1,3,5
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[bookmark: OLE_LINK1]Figure S10. N2 absorption/desorption isotherms and pore size distribution of the B-BTD-1,2,4,5
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