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Figure S1: Distribution of mean DO (mg L-1) as a function of the standard deviation of E-W velocity (m s-1) computed using a 24-hour moving window. Velocity was measured using an ADCP deployed near EXRK during July – August 2006. 
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