Highlights

· Reducing the rate of film formation can lead to an oriented distribution of CNT on the on the film surface and pore walls. 
· This study systematically investigates the impact of coating film thickness, structure, and coating process on the electromagnetic shielding performance of PVC-based composite films.
