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Figure S1 The viscosity values of casting solution of PVC/CNT composite films at different PVC concentrations.
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Figure S1 The viscosity values of casting solution of PVC/CNT composite films at different CNT concents.
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