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MOF/carboxymethylcellulose porous composite beads are synthesized in a simple one-step process. The lamellar interconnected structure not only facilitates the diffusion of contaminants in water but also provides good mechanical properties.
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