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TABLE S1 Experimental parameters for studied elements
	Element
	Wave length (nm)
	Slit (nm)
	HCL current (mA)

	Asa
	193.7
	0.7
	14

	Pbb
	217.0
	0.7
	12

	Cdb
	228.8
	0.7
	8

	Nib
	232.0
	0.2
	15


a - ETAAS, b - FAAS

TABLE S2. Temperature regime applied for the determination of As by ETAAS
	Step
	Temperature (°C)
	Time (s)
	Flow (L/min)

	1
	85
	5
	0.3

	2
	95
	40
	0.3

	3
	120
	20
	0.3

	4
	1400
	2
	0.3

	5
	1400
	1
	0.3

	6
	1400
	2
	0

	7
	2600
	0.6
	0

	8
	2600
	2
	0

	9
	2600
	2
	0.3





TABLE S3. Experimental parameters for studied elements
	Element
	slope
	intercept
	R2
	LOD (mg/kg)
	LOQ (mg/kg)

	Asa
	3.47E+00
	-4.50E-05
	0.9993
	0.01
	0.03

	Pbb
	5.84E-02
	-2.07E-04
	0.9978
	0.32
	0.98

	Cdb
	2.95E-01
	8.78E-04
	0.9978
	0.33
	0.99

	Nib
	7.86E-02
	-7.00E-04
	0.9981
	0.57
	1.74


a - ETAAS, b - FAAS

